
***Fuse*Fix HammerToe**



**Titanium**

**Solid & Cannulated Option Straight & Angled Option Integrated Instrument Design Sterile Packaged**

# Features and Benefits

The comprehensive FuseFix HammerToe was designed to provide the surgeon with speed of the procedure and accurate placement of the screw. The FuseFix HammerToe exhibits the following advantages:

* No additional instrumentation for a faster procedure
* Built in AO Connection
* Integrated instruments including drill & broach
* Barbed distal end for enhanced bone purchase and fixation
* Screws contain self-drilling and tapping features

Powered By

Phone: (972) 331-5900 [www.fusemedical.com](http://www.fusemedical.com/)

Please email [schedule@surgicalservice.com](mailto:schedule@surgicalservice.com) to place orders or schedule cases

# Implant - Ø2.0 Screw



|  |  |  |
| --- | --- | --- |
| **Ø2.0 Screw** | | |
| **Part #** | **Length** | **Description** |
| ***M*13-C20013** | **13mm** | FuseFix Cannulated Ø2.0mm x 13mm |
| ***M*13-S20013** | **13mm** | FuseFix Solid 0° Ø2.0mm x 13mm |
| ***M*13-S20113** | **13mm** | FuseFix Solid 10° Ø2.0mm x 13mm |

**Implant - Ø2.5 Screw**

|  |  |  |
| --- | --- | --- |
| **Ø2.5 Screw** | | |
| **Part #** | **Length** | **Description** |
| ***M*13-C25015** | **15mm** | FuseFix Cannulated Ø2.5mm x 15mm |
| ***M*13-S25015** | **15mm** | FuseFix Solid 0° Ø2.5mm x 15mm |
| ***M*13-S25115** | **15mm** | FuseFix Solid 10° Ø2.5mm x 15mm |

**Implant - Ø3.0 Screw**

|  |  |  |
| --- | --- | --- |
| **Ø3.0 Screw** | | |
| **Part #** | **Length** | **Description** |
| ***M*13-C30015** | **15mm** | FuseFix Cannulated Ø3.0mm x 15mm |
| ***M*13-S30015** | **15mm** | FuseFix Solid 0° Ø3.0mm x 15mm |
| ***M*13-S30115** | **15mm** | FuseFix Solid 10° Ø3.0mm x 15mm |



Powered By

Phone: (972) 331-5900 [www.fusemedical.com](http://www.fusemedical.com/)

Please email [schedule@surgicalservice.com](mailto:schedule@surgicalservice.com) to place orders or schedule cases